|  |  |  |
| --- | --- | --- |
| Algorithms | Percentage reduction | Remarks |
| PSO | 17.78 | The algorithm converged globally with minimum information exchange.  Load shifting technique |
| FA | 16 | More variation not suitable |
| SQP | 17.64 | More variation |
| GA | 14 | Heuristic-based load shifting technique |